**LAMPS**



**ATEX-EX** –Led lamp for zone 2, 21, 22



**ATEX-EX – Led lamp suitable for zone 2 (GAS) and 21 -22 (DUST)**

Waterproof led lamp in aluminium alloy EN1076 AC46001DF suitable for applications in risk of explosion areas as defined in ATEX Directive 94/9/EC. The body of the lighting fixture is treated with ecological anti-corrosion passivation with fluoro-zirconium and finished with hot polymerized scratch-resistant non-toxic polyester painting. The body colour is RAL 7035 light grey. The diffuser is in prismatic tempered glass. The protection cage is RAL 2011 deep orange and is attached to the body by means of stainless steel screws, the sealing is guaranteed by a gasket in non-ageing elastomer. Predisposed for entry through an M20 cable gland.

Complete with internal and external ground screw. Suitable for use in engine rooms

***Technical specifications*** ***Dimensions***

* Body material: aluminium alloy

 Diffuser material: prismatic tempered glass  Back box color: RAL 7035 light grey

 Protection cage color: RAL 2011 deep orange

* Emission angle: 120°
* Neutral white light
* DC power supply: 10…30 Vcc

 Protection rating: IP65  Insulation class: I

* Ambient temperature for use: -20…+40°C

 Cable section max: 2,5mm²

* Light intensity: 450 lux a 1 m

 Protected against power surges  Power consumption: 6 W

 Dimensions: 199 x 112 x 119mm

 Operative life: 30.000 hours at 25°C

|  |  |  |  |
| --- | --- | --- | --- |
| ***CONFORMITY TO STANDARDS*** |  | ***ATEX EXECUTION*** |  |
|  | ATEX Directive 94/9/CE |  | IIC 3G 2D - IP65 |  |
|  |  |  |
| ***Models*** | ***Description*** |  |  |
|  |  |
|  |  |  |
| **LAX120KW50** | Led lamp, surface frame, ATEX execution, neutral white, 10…30Vcc power supply |  |
| **LAX201152EX** | 2 poles Switches, 16A 250Vac, RAL 9005 (black), ATEX execution, IP66 protection rating |  |
| **LAX9XXKW50** | Led light bulbs, for watertight lighting fixture (ATEX Palazzoli), neutral white, 10…30Vcc p.supply |  |



Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 7

**LAMPS**



**LUXBOMA -** LED boom lamps, with courtesy light



**LUXBOMA, LED boom lamps with courtesy light**

LED lamps for the cockpit lighting. Elegant finishing, reduced dimensions, long duration and low power consumption.

Can be placed in the boom inferior groove (for ex. Selden™ and Sparcraft™). White main light and red courtesy one

Suitable also for assembly under crosstrees, rollbar and awnings on in motor vains

***Technical specifications*** ***Application***



* Case in anodized aluminum
* Emission angle 60°
* Cold white main light (5800°K)
* Red courtesy light
* Sea cable of 40 cm
* Power Supply: 10…30 Vdc
* High protection class IP66
* Luminous intensity: 450 lux at 1 m
* Protected against polarity inversion
* Protected against power surges
* Low power consumption (6 W), long duration
* Dimensions: 325 (Length) x 18 (A) x 18 mm (B)
* Work life: 30.000 hours @ 25°C



***Dimensions***



***Models*** ***Descriptions***

**LXB830KWR** Surface mount lamp, white light, red courtesy one

**AV0478** Mounting plastic clips (set of two)

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 8

**LAMPS**



**COURTESY LIGHTS**



**PERLA, LED courtesy lights for internals and externals**

Small and bright lights available in white, blue, red, green and amber. Designed for exterior use, with a single-piece case and fully resined inside, they are completely waterproof. They allow a simple and rapid installation and can be fixed with glue or screwed in and blocked with a nut. Useful for illuminating or marking steps, borders, ladders, bathrooms, cockpit area and other environments.

***Technical specifications*** ***Application***



* Polycarbonate case
* Emission angle 30°
* Models: white, blue, red, green and amber light
* Cable: 20 cm
* Power Supply: 10…30 Vdc
* High protection class IP67
* Luminous intensity: 20 lux 1 LED (1 m)
* No polarity
* Thread: 12 MA x 1,5 mm
* Low power consumption: 0,3 W (12V), 0,6W (24V)
* Dimensions: Ø 12 x 24 mm
* Work life: 30.000 hours @ 25°C

|  |  |  |  |
| --- | --- | --- | --- |
| ***Models*** | ***Description*** | ***Models*** | ***Description*** |
| **LPE112KW** | White courtesy light | **LPE112KA** | Amber courtesy light |
| **LPE112KB** | Blue courtesy light | **AV0411** | Chromed brass frame, Ø 24 x 6mm |
| **LPE112KR** | Red courtesy light | **AV0414** | Gilded brass frame, Ø 24 x 6mm |
| **LPE112KG** | Green courtesy light | **AV0454** | Line protection |

**GEMMA, LED courtesy lights for internals and externals**

Compact and bright lamps for exteriors. Available with light of colour white, blue, red, green or amber. With a single-piece case and fully resined inside, they are completely waterproof. They allow a simple and rapid installation and can be fixed anywhere with glue or screwed in and blocked with the nut. Useful for illuminating or marking steps, borders, ladders, cockpit area, bathrooms and other environments. They can be powered with any voltage between 10 and 30 Vdc..

***Technical specifications*** ***Application***

* Polycarbonate case
* Emission angle 30°
* Models: white, blue, red, green and amber light
* Cable: 20 cm
* Power Supply: 10…30 Vdc
* High protection class IP67
* Luminous intensity: 20 lux 1 LED (1 m)
* No polarity
* Thread: 12 MA x 1,5 mm
* Low power consumption: 0,3 W (12V), 0,6W (24V)
* Dimensions: Ø 18 x Ø 12 x 24 mm
* Work life: 30.000 hours @ 25°C



|  |  |  |  |
| --- | --- | --- | --- |
| ***Models*** | ***Description*** | ***Models*** | ***Description*** |
| **LGE118KW** | White courtesy light | **LGE118KG** | Green courtesy light |
| **LGE118KB** | Blue courtesy light | **LGE118KA** | Amber courtesy light |
|  |  |  |  |
| **LGE118KR** | Red courtesy light | **AV0391** | Stainless frame, dim. Ø 32 x 4mm |

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 9

**LAMPS**



**GIADA -** LED lamp for interiors



**GIADA, LED lamps for interiors**

New-concept minimal design, based on LED technology. Light emission is wide and uniform. Designed to be used on work panels, engine rooms, lifts, kitchens and wardrobes. Models available, with or without onboard power switch. Their low power consumption makes them useful for emergency scenarios, powered by a battery.

***Technical specifications*** ***Application***



* High brightness, bright light
* Aluminum and plastic case
* Neutral white light (4500 °K)
* Emission angle: 120°
* Opaline filter
* Power Supply: 10…30 Vdc
* Luminous intensity: 80 lux 1 m
* No polarity
* Protection class: IP42
* Protected against power surges
* Low power consumption: 6 W
* Work life: 30.000 hours @ 25°C
* Dimensions: 240 (A) x 70 (C) x 35mm (B)

***Dimensions***



***Models*** ***Description***

**LGD114KW** LED lamp for internals, without switch, opaline front filter.

**LGD214KW** LED lamp for internals, with switch, opaline front filter

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 10

**LAMPS**



**LED MODULAR LAMPS**



PRISMA



SIBILLA

**PRISMA/SIBILLA, LED modular lamps for interiors and exteriors**

Suitable to light ambients, as kitchen, baths, cabinets, motor vains, lockers, cockpits and awnings. Suitable where it is useful to have strong lamps, of minimum size, long duration and low consumption

|  |  |  |  |
| --- | --- | --- | --- |
| ***Technical specifications*** | ***PRISMA*** | ***SIBILLA*** |  |
|  | 4 standard sizes |  |  |  |
|  Neutral white light: 5000 °K |  |  |  |
|  Emission angle 90° Prisma |  |  |  |
|  Emission angle 120° Sibilla |  |  |  |
|  | Power supply: 12 o 24 Vdc |  | ***AV0425*** |  |
|  |  |  |  |

* Prisma light intensity: 310 lux 1 m (530 lux double density)



|  |  |  |
| --- | --- | --- |
|  | Sibilla light intensity: 280 lux 1 m (480 lux double density) | ***AV0428*** |
|  | IP54 plastic case |  |
|  | Protected against power surges | ***AV0426*** |

* Prisma dimensions: 12,5 (A) x 10,5mm (B) x 220…99 0 mm
* Sibilla dimensions: Ø 14mm x 220…990 mm
* Set of two metal or plastic clasps for mounting



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***Models*** | ***Description*** | ***Length*** | ***Consumption*** | ***N° led’s*** |
| **LPI122FW40** | LED lamp, 12 Vdc | 220mm | 3,2 W | 12 |
| **LPI151FW40** | LED lamp, 12 Vdc | 510mm | 8 W | 30 |
| **LPI171FW40** | LED lamp, 12 Vdc | 710mm | 11,2 W | 42 |
| **LPI199FW40** | LED lamp, 12 Vdc | 990mm | 16 W | 60 |
|  |  |  |  |  |
| **LPI227FW40** | LED lamp, 12 Vdc, double density | 270mm | 8 W | 30 |
| **LPI251FW40** | LED lamp, 12 Vdc, double density | 510mm | 16 W | 60 |
| **LPI277FW40** | LED lamp, 12 Vdc, double density | 770mm | 24 W | 90 |
| **LPI299FW40** | LED lamp, 12 Vdc double density | 990mm | 32 W | 120 |
|  |  |  |  |  |
| **LSI122FW40** | LED lamp, 12 Vdc | 220mm | 3,2 W | 12 |
| **LSI151FW40** | LED lamp, 12 Vdc | 510mm | 8 W | 30 |
| **LSI171FW40** | LED lamp, 12 Vdc | 710mm | 11,2 W | 42 |
| **LSI199FW40** | LED lamp, 12 Vdc | 990mm | 16 W | 60 |
|  |  |  |  |  |
| **LSI227FW40** | LED lamp, 12 Vdc, double density | 270mm | 8 W | 30 |
| **LSI251FW40** | LED lamp, 12 Vdc, double density | 510mm | 16 W | 60 |
| **LSI277FW40** | LED lamp, 12 Vdc, double density | 770mm | 24 W | 90 |
| **LSI299FW40** | LED lamp, 12 Vdc, double density | 990mm | 32 W | 120 |

|  |  |  |  |
| --- | --- | --- | --- |
| ***Models*** | ***Options*** | ***Models*** | ***Accessories*** |
|  |  |  |  |
| **G** | 24 Vdc power supply | **AV0425** | Set of two metal clasps for mounting |
| **30** | Warm white light 3000°K | **AV0426** | Set of two plastic clasps for mounting |
|  |  | **AV0428** | Set of two plastic clasps for mounting |

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 11

**LAMPS**



**SPOT -** LED light bulbs



**SPOT 28, LED lamps, diameter 28 mm, for G4 and GU 5.3 sockets**

High efficiency LED lamps. They replace the halogen lamps from 15 W and offer a consumption of only 2,2 W with an operating life 10 times superior. They emit a pleasant warm white light (very similar to the halogen one) that is given out in uniform way in the environment thanks to the wide and uniform emission angle.

The available model satisfies different needs of Power Supply and connection.

***Technical specifications*** ***Dimensions***

* Replace the halogen bulbs from 15W
* Bulb diameter: 28 mm
* G4 and GU5.3 sockets (central, changeable in

lateral surface)

 Warm white light (3000 °K), CRI80  Emission angle 120°

 Power Supply: 10…30 Vdc

* Luminous intensity: 40 lux at 1 m (11 lux-2m)
* No polarity
* Protected against power surges
* Low power consumption 2,2 W
* Dimensions: 28 (A) x 30 (B) x 8 mm (C)
* Work life: 30.000 hours @ 25°C

|  |  |  |  |
| --- | --- | --- | --- |
| ***Models*** | ***Description*** | ***Models*** | ***Accessories*** |
| **LSP28CKW30** | LED lamp, socket G4/GU5.3 central, 10÷30Vdc | **AV0454** | Line protection |
|  |  |  |  |

**SPOT 35, LED lamps, diameter 35mm, for G4 and GU 5.3 sockets, with dimmer**

High efficiency LED lamps. They replace the halogen lamps from 20 W and offer a consumption of only 3 W. They emit a pleasant warm white light (very similar to the halogen one) that is given out in uniform way in the environment thanks to the wide and uniform emission angle.

The available model satisfies different needs of Power Supply and connection.

***Technical specifications*** ***Dimensions***

* Replace the halogen bulbs from 20W
* Bulb diameter: 35 mm



 G4 e GU5.3 sockets (central, changeable in lateral surface)



 Warm white light (3000 °K), CRI80  Emission angle 120°

 Power Supply: 10…30 Vdc

 Luminous intensity: 55 lux at 1 m (15 lux-2 m)

* Protected against power surges
* Low power consumption 3 W
* Dimensions: 35 (A) x 30 (B) x 8 mm (C)
* Work life: 30.000 hours @ 25°C

|  |  |  |  |
| --- | --- | --- | --- |
| ***Models*** | ***Description*** | ***Models*** | ***Accessories*** |
| **LSP35CKW30** | LED lamp, sockets G4/GU5.3 central | **ACD003** | Dimmer, 100 W (12 Vdc) |
|  |  |  |  |
| **LSP35CKW30D** | LED lamp, sockets G4/GU5.3 central, dimmable | **AV0454** | Line protection |
|  |  |  |  |

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 12

**LAMPS**



**SPOT -** LED light bulbs



**SPOT 50, LED lamps, diameter 50 mm, for internal and external use**

High protection and efficiency LED lamps. They replace the halogen lamps from 20 W and offer a power consumption of only 3 W with an operative life 10 times superior. They emit a pleasant warm white light (very similar to the halogen one) that is given out in uniform way in the environment thanks to the wide and uniform emission angle. Suitable also to be installed in external environments (option S).

***Technical specifications*** ***Dimensions***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  Diameter 50mm, wires connection |  |  |
|  |  |  Low power consumption: 3 W |  |  |  |
|  |  |  Warm white light: 3000 °K (neutral 4000°K) |  |  |  |
|  |  |  | Emission angle 120° |  |  |  |
|  |  |  Dimmable models (Dimmer ACD003) |  |  |  |
|  |  |  | Satinized front filter |  |  |  |
|  |  |  Power Supply: 12 Vdc/ac,10÷30 Vdc |  |  |  |
|  |  |  Protection class IP40 (IP65 option S) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  Luminous intensity: 55 Lux-1m (15 at 2m) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  Protected against power surges |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  Work life: 30.000 hours at 25°C |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | Dimensions: 50 (A) x 22 (B) x 43mm (C) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  Recessed hole: Ø 46 (option version “M”) |  |  |
| ***Models*** | ***Description*** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **LSP50FJW30** | LED lamps for internals, 12 Vdc/ac, warm white light (3000°K) |  |  |
| **LSP50FKW40** | LED lamps for internals, 10..30 Vdc, neutral white light (4000°K) |  |  |
| **LSP50FKW30D** | LED | lamps for internals10..30 Vdc,, warm white light (3000°K), dimmerable |  |  |
| **LSP50FKW40D** | LED | lamps for internals, 10..30 Vdc, neutral white light (4000°K), dimmerable |  |  |
| **S** | Protection cap (IP65), for external use |  |  |
| **M** | Springs for the recessed insertion (not compatible with the option “S”) |  |  |



**SPOT MR16, LED lamps, diameter 50mm, with GU5.3 socket, for internals**

LED lamps with high efficiency, same size of the dichroic 20 W halogen ones, but have a power consumption of only 3W with an operative life 10 times superior. They emit warm white light (similar to the halogen) given out in uniform way in the environment thanks to the wide emission angle.

***Technical specifications*** ***Dimensions***

* Lamps equal to the halogen ones by 20 W

 Diameter: 50 mm, with socket GU5.3  Warm white light (3000 °K)

 Emission angle 120°  Satinized filter

 Power Supply: 12 Vdc/ac

 Luminous intensity: 55 lux at 1 m (15 lux 2m)



* No polarity

 Protected against power surges

* Low power consumption 3 W

 Dimensions: 50 (A) x 47 (B) x 44mm (C)  Work life: 30.000 hours at 25°C

***Models*** ***Description***

**LSPM16JW30** LED lamp, GU5.3 socket, 12 Vdc/ac

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 13

**LAMPS**



**ZEN -** LED spotlights, recessed mount, for interiors



**ZEN 45, LED spotlights, recessed mount, for interiors (transparent filter)**

Essential and minimum size, very thin. Suitable for classic and modern environments. Chromed plastic frame. Suitable to light closets, kitchens or as courtesy lights.

The low consumption allows to use them in high autonomy emergency plants.

They offer a simple and quick installation; they can be fastened under pressure or with the nut.

***Technical specifications***

Transparent filter



Map filter



* Equivalent to the halogen ones by 15W
* Low power consumption: 2,2W (9 LED)
* Power Supply: 10…30 Vdc
* Emission angle 120°
* Neutral white light (4000°K)
* Luminous intensity: 33 lux at 1 m (13 lux at 2 m)
* No polarity and protected against power surges
* Recessed mounting: pressure fastening or with the die
* Wires connections from 30cm
* Protection class: front IP66, back IP40
* Dimensions: 45 (A) x 19 (C) x 40,8 mm (B), hole Ø 41,0 mm
* Work life: 30.000 hours at 25°C

**Dimensions**



|  |  |  |
| --- | --- | --- |
| ***Models*** | ***Description*** |  |
| **LZE45KW40T** | 9 LED spotlight, Ø 45mm, hole Ø 41mm, 2 wires, 10…30 | Vdc, neutral white light, transparent filter |
| **LZE45KW40L** | 9 LED spotlight, Ø 45mm, hole Ø 41mm, 2 wires, 10…30 | Vdc, neutral white light, map filter |

**ZEN 45, LED spotlights, recessed mount, for interiors bicolored**

Essential and minimum size, very thin. Chromed plastic frame. Suitable to light throughfare or as courtesy lights, two-colors. They offer a simple and quick installation; they can be fastened under pressure or with the nut.

***Technical specifications***

 Low consumption: 1 W (9 LED)  Power Supply: 10…30 Vdc

 Emission angle 120°  White and blue light

 Protected against polarity inversion  Protected against power surges

 Recessed mounting: hole Ø 41mm, pressure fastening or with the die  Wires connections from 30cm

 Protection class: front IP66, back IP65

 Dimensions: 45 (A) x 19 (C) x 40,8 mm (B), hole Ø 41,0 mm

***Models*** ***Description***

**LZE45KWB** LED spotlight, Ø 45mm, 10…30 Vdc,, white light and bl ue courtesy light, map filter

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 14

**LAMPS**



**SABA -** LED spotlights, recessed mount, stainless



***Application***



**SABA, LED spotlights, recessed mount, s.steel frame, for interiors and exteriors**

Elegant stainless steel structure AISI 316. Intense and uniform lighting with a wide emission angle. Suitable for classic and modern environments. Standard gloss finish or satin (option). Suitable to light cabins, kitchens, cockpit, baths, integrated directly in the furniture, motor vain. Their low power consumption allows them to be used in emergency setups.

***Technical specifications*** ***Dimensions***

* Stainless steel AISI 316 case
* Equivalent to halogen spotlights of 20 W

 Emission angle 120°



* Matte filter

 Warm white light (3000°K) or Neutral white light (4000°K)  Low power consumption: 3 W



* Power Supply: 12 Vdc/ac

 Power Supply: 10…30 Vdc, also with dimmer (ACD001/ 3)

* Protection class: IP52 front, IP20 back
* Usable also to the external: with S option (IP65)

 Luminous intensity: 55 Lux at 1m (15 Lux at 2m)  Protected against power surges

 Recessed mounting, with spring fastening

* Dimensions: 78 (A) x 62 (B) x 30 (C) x 8mm (D)
* Work life: 30.000 hours at 25°C

|  |  |
| --- | --- |
| ***Models*** | ***Description*** |
| **LSA80RJW30** | LED spotlight, bright finishing, Power Supply 12 Vdc/Vac, Warm white light |
| **LSA80RKW40** | LED spotlight, bright finishing, Power Supply 10…30 Vdc , Neutral white light |
| **LSA80RKW30D** | LED spotlight, bright finishing, Power Supply 10…30 Vdc , Warm white light , with dimmer |
|  |  |
| **LSA80RKW40D** | LED spotlight, bright finishing, Power Supply 10…30 Vdc , Neutral white light , with dimmer |
|  |  |
| **B** | Satinized finishing |
| **S** | Treatment for IP65 external use |
| **ACD001** | Dimmer for loads up to 25 W (12 Vdc) – 50 W (24 Vdc) |
| **ACD003** | Dimmer for loads up to 100 W (12 Vdc) – 200 W (24 Vdc) |
| **AV0454** | Line protection |

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 15

**LAMPS**



**PUNTO -** Recessed LED spotlight for interiors



**PUNTO, Recessed LED spotlight for interiors**

Compact and elegant, they are suitable for classic and modern rooms. Alluminium alloy frame with chromium-plated finish (on request white or golden). They are suitable for lift cars, elevator shafts and engine rooms. The Low power consumption allows to use them in high autonomy emergency plants. They are also available pre-cabled for fast hooking/unhooking..

***Technical specifications*** ***Dimensions***

* Corresponding to 20 W halogen spotlight

 Low power consumption 3 W

 Two power supply types: 12 Vdc/ac, 10…30 Vdc

* Emission angle 120°
* Warm white light (3000°K) or neutral (4000°K)
* Lighting intensity 55 Lux at 1 m, 15 Lux at 2 m
* Without polarity, Protected against power surges

 Cable with connector for fast hooking/unhooking (P option)  Recessed mount, with spring fastening

* Dimensions LPT75 models: 75 (A) x 65 (C) x 30mm (B)
* Dimensions LPT60 models: 60 (A) x 48 (C) x 30mm (B)
* Protection class IP40 (IP65 with S option)
* Operative life: 30.000 hours at 25°C

***Pre-cabled system***



|  |  |  |  |
| --- | --- | --- | --- |
| ***Models*** | ***Description*** | ***Models*** | ***Description*** |
| **LPT75JW30** | LED spotlight, 12 Vdc/ac, Warm white | **P** | Connettor on the power supply cable |
| **LPT75KW40** | LED spotlight, 10÷30 Vdc, neutral white | **S** | Treatment for protection IP65 |
| **LPT60KW40T** | LED spotlight, 10÷30 Vdc, neutral white | **AV0424** | Extension 1200mm |
| **D** | Frame golden finishing | **AV0454** | Line protection |
| **W** | Frame white finishing | **AV0438** | Power supply 100-240 Vac / 12 Vdc, 25 W |

Binding Union srl – via Cuorgnè, 21 – 10156 Torino – Italy – tel. +39.011.2625414 – Fax +39.011.2625428 –www.binding.it – 16